\documentclass[12pt]{article}
\evensidemargin=-.2in
\oddsidemargin=-.2in
\textwidth=7.4in
\pagestyle{empty}
\topmargin=-0.8in
\headheight=0in
\headsep=0in
\parindent=0in
\textheight=11.1in

\newcommand{\rulew}[1]{\rule{#1}{.01in} }
\newcommand{\bc}{$\bigcirc$}
\newcommand{\tabul}{\<\rule[-0.035in]{7.5in}{.01in}\>}

\begin{document}
\begin{center}
\end{center}
T5 Checklist, Version 24, \today \hfill Signature: 
\rulew{2in} \\

Operators: \rulew{2.4in} Date: \rulew{.6in} Time: \rulew{.6in} Shot
 \#: \rulew{1.1in} \\
Notes: \rulew{6.9in}
\hrule 
\bigskip
\smallskip
\hrule


\smallskip
Piston Mass: \rulew{1in} kg
\hrule

\vspace{-.1in}
\begin{tabbing}
\=\hspace{1in}\= \hspace{3in} \+ \kill
Diaphragm \> Thickness: \rulew{1.5in} \\
\tabul \> Expected burst pressure: \rulew{0.8in} MPa \hspace{.2in} Value: \rulew{0.8in} MPa \\
\=\hspace{2.5in}\= \hspace{3.5in}\= \hspace{.5in} \= \+ \kill
Position Tunnel correctly \> LVDT1: setting: \rulew{.5in} value: \rulew{.5in}
 \> $\bigcirc$ \\
\tabul \> LVDT2: setting: \rulew{.5in} value: \rulew{.5in} \> $\bigcirc$ \> A \\
\= \hspace{.45in}\= \hspace{5.55in}\= \hspace{.5in}\= \+ \kill
Turn off blower                                    \> \> \bc \\
Open  \> SV-24 (DT pressure gage)                     \> \bc \\
      \> SV-23 (DT vacuum gage)                       \> \bc \\
      \> HS-20 (DT vacuum pump isolation valve)       \> \bc \\
Close \> HS-19 (DT vacuum pump vent)                  \> \bc \\
      \> HS-21 (DT vent)                              \> \bc \\
Turn on cooling water for DT pump                  \> \> \bc \\
\tabul Turn on PO/3 (DT vacuum pump)               \> \> \bc \\
Open  \> V-17 (ST vacuum valve)                       \> \bc \\
Close \> V-18 (ST vacuum pump vent valve)             \> \bc \\
Turn on PO/2 (ST vacuum pump)                      \> \> \bc \\
Open  \> SV-25A (ST pressure gage)                    \> \bc \\
      \> SV-25B (ST pressure gage)                    \> \bc \\
      \> SV-26 (ST vacuum gage)                       \> \bc \\
\tabul\> V-14a, V-14b, V-14c (ST Isolation Valves)           \> \bc \\
Close \> 2R pressure isolation valve (near P1)        \> \bc \\
Open  \> V-11 (High pressure CT isolation)            \> \bc \\
      \> V-8 (CT vacuum)                              \> \bc \\
      \> V-7 (CT/2R vacuum valve)                     \> \bc \\
      \> V-12 (CT/2R/PS vacuum valve)                 \> \bc \\
Close \> ZS-4 manual and remote (emergency 2R vent)   \> \bc \\
      \> ZS-13 (CT vacuum pump vent valve)            \> \bc \\
Turn on PO/1 (2R, Piston Space and CT vacuum pump) \> \> \bc \\
Open  \> SV-29 (CT vacuum gage)                       \> \bc \\
      \> SV-27 (2R vacuum gage)                       \> \bc \\
      \> SV-31 (PS vacuum gage)                       \> \bc \> D \\
Open CT gauge(s)                                   \> \> \bc \\
Flex Hose: (Top valve closed)(Bot valve Open)      \> \> \bc \\
\hspace{.45in}\= \hspace{5.55in}\= \hspace{.5in}\= \kill
\tabul \> Wait 30 - 60 minutes for vacuum \> \bc \\
\hspace{4in}\= \hspace{2in}\= \kill
WARNING LIGHTS ON (P1). Verify door is closed \> \> \bc \\
Check vacuum levels \> DT:\' \rulew{1in} mmHg \> \bc \\
                    \> ST:\' \rulew{1in} mmHg \> \bc \\
                    \> CT:\' \rulew{1in} mmHg \> \bc \\
                    \> 2R:\' \rulew{1in} mmHg \> \bc \\
\tabul \> PS:\' \rulew{1in} mmHg \> \bc \\
\hspace{6in}\= \kill
Disconnect nozzle support trolley \> \bc \\
Isolate ST vacuum valve (V-17)    \> \bc \\
Turn off ST vacuum pump (PO/2)    \> \bc \\
Open ST vacuum pump vent valve (V18) \> \bc \\
\tabul Isolate ST vacuum gauge (SV-26)      \> \bc \\
\hspace{6in}\= \kill
Close V-14a (ST vac pump isolation) \> \bc \\
Close V-14b (ST vac gauge isolation \> \bc \\
\end{tabbing}
\newpage

\begin{tabbing}
\=\hspace{.45in}\= \hspace{5.55in}\= \hspace{.5in}\= \+ \kill
\tabul \\
\tabul \> \hspace{2in} Action \> Check \> \hspace{.2in} Signal \\
\=\hspace{1.8in}\= \hspace{1in}\= \hspace{1.2in}\= 
                                    \hspace{2.2in}\=\hspace{.5in}\= \+ \kill
Fill ST \> gas: \rulew{1in} \> \> setting:\' \rulew{1in} kPa absolute 
 \> \bc \\
 \> \> \> (multiply setting by 20) thumbwheel:\' \rulew{1in} \> \bc \\
 \> \> \> \hspace{1.5in} value:\' \rulew{1in} \> \bc \\
Press hand switch HS-C3 to confirm ST pressure \> \> \> \> \bc \\
\tabul Close V-14c (Fill line isolation)               \> \> \> \> \bc \\
Isolate DT pressure gauge, HS-24               \> \> \> \> \bc \\
Close ZS-20 (DT vacuum isolation)              \> \> \> \> \bc \\
Turn off HS-3 (dump tank vacuum pump)          \> \> \> \> \bc \\
Open vent HS-19 (DT vacuum pump vent)          \> \> \> \> \bc \\
Close V-8 (CT isolation)                       \> \> \> \> \bc \> E \\
Close (ST gages): \> SV-25A  \&  \> SV-25B           \> \> \bc \> F \\
\tabul Close SV-29 (CT vacuum gage)            \> \> \> \> \bc \> G \\
Fill CT \> gas: \rulew{1in} \> \> vacuum:\' \rulew{1in} kPa gage \\
        \>                  \> \> setting:\' \rulew{1in} kPa absolute \\
        \>                  \> \> thumbwheel:\' \rulew{1in} kPa gage \\
        \>                  \> \> value:\' \rulew{1in} kPa gage \> \bc \\
Absolute presure desired: \rulew{1.5in} \\
        \> gas: \rulew{1in} \\
        \>                  \> \> setting:\' \rulew{1in} kPa absolute \\
        \>                  \> \> thumbwheel:\' \rulew{1in} kPa gage \\
        \>                  \> \> value:\' \rulew{1in} kPa gage \> \bc \\
\tabul Close V-11 (CT high pressure isolation valve) \> \> \> \> \bc \> H \\
Close V-7 (CT/2R vacuum)             \> \> \> \> \bc \\
\tabul Close SV-23 (DT vacuum gage)  \> \> \> \> \bc \> I,J \\

Close SV-27 (2R vacuum gage)         \> \> \> \> \bc \\
2R Temperature before \rulew{1in}$^{\rm o}$C \> \> \> \> \bc \\
Fill 2R:  \>                \> \> setting:\' \rulew{1in} PSI gage \\
          \>                \> \> thumbwheel:\' \rulew{1in} PSI gage \\
\tabul    \>                \> \> value:\' \rulew{1in} PSI gage \> \bc \\
Check for changes in tunnel position CT: 
                 \rulew{.5in} CT-2R: \rulew{.5in} \hspace{1.35in} \bc \\
Desired tunnel position \hspace{.889in} CT: \rulew{.5in} CT-2R: \rulew{.5in} \hspace{1.35in} \bc\\
Toggle Dry Run Relay box to ``Experiment'' \> \> \> \> \bc \\
\tabul Arm ``T5 das''                       \> \> \> \> \bc \\
Isolate flex hose (bottom valve)                    \> \> \> \> \bc \\
Confirm 2R pressure, Hand switch HS-C1 \> \> \> \> \bc \\
Isolate 2R gage                        \> \> \> \> \bc \\
\tabul Confirm isolation, Hand switch HS-28   \> \> \> \> \bc \> K,L \\
\tabul Close SV-31 (PS vacuum gage)    \> \> \> \> \bc \> M \\
\tabul Confirm CT pressure, Hand switch HS-C2 \> \> \> value:\' \rulew{1in}
  kPa gage \> \bc \> N \\
Isolate CT gage                        \> \> \> \> \bc \\
Confirm isolation, Hand Switch HS-30 \> \> \> \> \bc \> O \\
\tabul 2R Temperature after \rulew{1in}$^{\rm o}$C \> \> \> \> \bc \\
Close V-12 (2R vacuum)                      \> \> \> \> \bc \> P \\
Open V-13 to vent CT vacuum pump            \> \> \> \> \bc \\
Turn off CT vacuum pump (PO/1)              \> \> \> \> \bc \\
READY TO FIRE \> \> \> Time:\'\rulew{1in} \> \bc \\
\tabul Press and hold down firing buttons   \> \> \> \> \bc \\
\tabul Make the Tunnel Safe          \>\>     \> \> \bc \\
Open  \> V-4                       		\>\>								\> \bc \\
Open  \> Flex Hose Isolation Valves         \>\>    			\> \bc \\
Reconnect nozzle support trolley \>\>\>\> \bc \\
\end{tabbing}
\end{document}
